I am interested in a road marking machine from STRAMAT Vertriebs GmbH.

It has to fulfill the following conditions. 

We would like to carry out the following road marking work:
- Parking lot markings
- Road markings in the municipal area
- Extensive road markings in urban areas
- Road markings on rural roads
- Road markings on highways
- Ground markings on airfields
- Floor markings in industrial halls
- Floor markings on race tracks

The road marking machine should be able to process the following marking materials:
- 1 K paints (high-solid paints)
- Epoxy-modified high-solid paints
- Spray plastics 98:2
- Spray plastics 1:1
- Marking paints for race tracks (FIA-compliant)
- Cold plastics
- Polyurethane paints

Application of reflective glass beads
- The road marking requires a device for applying reflective glass beads
- The road marking does not require a device for applying reflective glass beads

The road marking machine must be capable of the following marking technique:
- Application with airless technology
- Application with airspray technology
- Application with cold plastic systems

The road marking machine should have the following power source:
- Internal combustion engine
- Electric drive

The machines should have the following drive:
- Hand-guided road marking machine
- Hand-guided road marking machine with detachable drive carriage
- Road marking machine with its own hydraulic drive
- Ride-on road marking machine with hydraulic drive

The road marking machine should have a control system with the following specifications:
- Automatic line/gap control
- Delayed reflective glass bead spreader
- Color display
- Personalized display
- Speed display
- Display of pump pressure
- Control of the average applied wet film thickness
- Recording of distances traveled
- Recording of marked distances
- Recording of temperature and humidity data
- Telematics function for the transmission of activities carried out
- The control system must be multilingual
- The control system must be self-explanatory

Create a selection of at least 4 potential products.